(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(J1-Pin_1)")
  (net 2 "Net-(J1-Pin_2)")
  (net 3 "/Yoman/A")
  (net 4 "/Yoman/B")
  (net 5 "/Yoman3/C")
  (net 6 "/Yoman/C")
  (net 7 "/Yoman1/C")
  (net 8 "/Yoman2/C")

  (footprint "Connector_Harwin:Harwin_M20-89004xx_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tstamp 5d5b4734-2f28-4a66-b73c-d81d95c57109)
    (at 185.07 115.79)
    (descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89004xx, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
    (tags "connector Harwin M20-890 horizontal")
    (property "Sheetfile" "WillItBlend.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (path "/693d932e-04b3-4f70-8a85-56b4904b7bed")
    (attr smd)
    (fp_text reference "J1" (at -0.48 -6.28) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e89e1913-364b-4aaa-addb-fd798d33b540)
    )
    (fp_text value "Conn_01x04_Pin" (at -0.48 6.28) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25e364b7-8a70-447b-89ca-b9b36e2e3312)
    )
    (fp_text user "${REFERENCE}" (at -0.48 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee901389-bf45-4d15-af75-701c887926a0)
    )
    (fp_line (start -7.095 -4.63) (end -5.525 -4.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c757387-ed84-4810-87b4-5250ff827543))
    (fp_line (start -7.095 -3.81) (end -7.095 -4.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aea88551-93f8-4886-9cbd-0d45ab09149d))
    (fp_line (start -3.955 -4.25) (end -1.845 -4.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d634e0d0-18e3-41c8-9b16-2eec2de89e4e))
    (fp_line (start -3.955 -3.37) (end -1.845 -3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec82c7d5-d093-4b9c-91a8-9d0052c1c836))
    (fp_line (start -3.955 -1.71) (end -1.845 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc93dd47-9eca-4505-b61a-6ac5e6a2a99f))
    (fp_line (start -3.955 -0.83) (end -1.845 -0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 731936a8-8b38-4b1a-a697-833dd18758bd))
    (fp_line (start -3.955 0.83) (end -1.845 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8cc553b-a040-4d84-b84b-418bd92804ee))
    (fp_line (start -3.955 1.71) (end -1.845 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c00c22a-5eeb-4704-a54f-372a9c8c68cc))
    (fp_line (start -3.955 3.37) (end -1.845 3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5bbf1646-4fd9-4871-956b-94a6be261627))
    (fp_line (start -3.955 4.25) (end -1.845 4.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d5756bc-11ca-465d-8e80-48a1c7afc23d))
    (fp_line (start -1.845 -5.2) (end 0.895 -5.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb344277-01ae-4908-b8e4-33f6af205404))
    (fp_line (start -1.845 5.2) (end -1.845 -5.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4afcbf55-3dd0-458d-a706-fa483b9e0326))
    (fp_line (start 0.895 -5.2) (end 0.895 5.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ed65577-238b-4cd4-8e5c-0267cf91192b))
    (fp_line (start 0.895 -4.25) (end 6.895 -4.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 13618d35-0ed5-4df8-8545-6e686d2ea7d4))
    (fp_line (start 0.895 -1.71) (end 6.895 -1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f5811ab-5b38-499d-8bd0-901317aa0205))
    (fp_line (start 0.895 0.83) (end 6.895 0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce4aad3a-6e37-4bb4-b71b-89cd2b8d19a0))
    (fp_line (start 0.895 3.37) (end 6.895 3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fd013f72-4b7b-4049-a89f-2654d6dffe4d))
    (fp_line (start 0.895 5.2) (end -1.845 5.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83e3412c-d52a-4e03-974e-84736ed8db82))
    (fp_line (start 6.895 -4.25) (end 6.895 -3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab32b117-6144-494f-a7d3-407c660db434))
    (fp_line (start 6.895 -3.37) (end 0.895 -3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c380883a-e4be-4d9e-80c1-77e9dc302135))
    (fp_line (start 6.895 -1.71) (end 6.895 -0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6033b9b-240e-40ed-8723-a62a9940cd6a))
    (fp_line (start 6.895 -0.83) (end 0.895 -0.83)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 820618c5-b37a-4e1a-b148-e19c12d00c67))
    (fp_line (start 6.895 0.83) (end 6.895 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5926b30a-e394-46be-8b8d-12c235a457cc))
    (fp_line (start 6.895 1.71) (end 0.895 1.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 20ea7d2a-63b5-4f3d-acab-bd400c280dcd))
    (fp_line (start 6.895 3.37) (end 6.895 4.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 70e131a6-5347-402c-93e8-e0538cece05e))
    (fp_line (start 6.895 4.25) (end 0.895 4.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b1f2875-195b-4099-a90d-7bb116b66799))
    (fp_line (start -7.28 -5.58) (end 7.28 -5.58)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b4a503b6-e46f-4007-9b7b-6f321b19ab50))
    (fp_line (start -7.28 5.58) (end -7.28 -5.58)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a636664-1165-423f-b8af-63472eef50f7))
    (fp_line (start 7.28 -5.58) (end 7.28 5.58)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 10918d16-0224-4144-9c9e-28c92b3228d5))
    (fp_line (start 7.28 5.58) (end -7.28 5.58)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b06c7239-56ff-49dd-b2db-9303a5f370fd))
    (fp_line (start -6.425 -4.13) (end -6.425 -3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77b12af9-2229-4678-856c-ca3f3c512c66))
    (fp_line (start -6.425 -3.49) (end -1.725 -3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8bae19e4-395f-4bc7-bb92-2b6cb5514ab0))
    (fp_line (start -6.425 -1.59) (end -6.425 -0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1481e6d4-f1d7-47d6-b327-a5ce5786a1ef))
    (fp_line (start -6.425 -0.95) (end -1.725 -0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c6b77fbd-1fca-4a1e-8ec0-29cd5de7855d))
    (fp_line (start -6.425 0.95) (end -6.425 1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp feebc3bd-6597-4b32-8fc1-2f4f3c54bc5f))
    (fp_line (start -6.425 1.59) (end -1.725 1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 17a08ada-0884-484a-b8a1-9694f936aa7a))
    (fp_line (start -6.425 3.49) (end -6.425 4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 50bfd7ea-6aa3-4342-b153-ff445a6c94f1))
    (fp_line (start -6.425 4.13) (end -1.725 4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1a99ae4-e40b-491f-bbd4-33e3298e8707))
    (fp_line (start -1.725 -4.68) (end -1.325 -5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0bb129dc-9eb3-437f-a9e4-315b4684c037))
    (fp_line (start -1.725 -4.13) (end -6.425 -4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e6a0db3-92c7-470d-84b6-b21bc5a1165e))
    (fp_line (start -1.725 -1.59) (end -6.425 -1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d7acb956-237b-40f4-a0ac-6d2bb4dc08e6))
    (fp_line (start -1.725 0.95) (end -6.425 0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cbe73dab-ba6f-4d3d-a7bc-7ddd3600adbb))
    (fp_line (start -1.725 3.49) (end -6.425 3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1aea7366-d48e-4c92-b460-fa729d7e3b4e))
    (fp_line (start -1.725 5.08) (end -1.725 -4.68)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a864c5bc-a305-44ae-aca2-156e52b0ae9d))
    (fp_line (start -1.325 -5.08) (end 0.775 -5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 120a2fa0-1d4b-442c-8e14-8e90c94692bc))
    (fp_line (start 0.775 -5.08) (end 0.775 5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b10cccb-a376-4b6d-88ac-0e50276ab9ca))
    (fp_line (start 0.775 -4.13) (end 6.775 -4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c262c6ac-debc-41eb-9ff4-fe76e7452a2b))
    (fp_line (start 0.775 -1.59) (end 6.775 -1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 01a9c581-9ea4-4958-8ef0-e5b64be562dd))
    (fp_line (start 0.775 0.95) (end 6.775 0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5cab803-2115-43f1-bfce-ca81c235bbc4))
    (fp_line (start 0.775 3.49) (end 6.775 3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09606cb9-a94e-491a-9da7-b8e19715bbb6))
    (fp_line (start 0.775 5.08) (end -1.725 5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c6600aa-cd14-4c51-8b37-160696d73985))
    (fp_line (start 6.775 -4.13) (end 6.775 -3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec8733ab-db85-4c23-981d-01220b359124))
    (fp_line (start 6.775 -3.49) (end 0.775 -3.49)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c2d93896-ec0b-4a92-a04e-e7e4da806921))
    (fp_line (start 6.775 -1.59) (end 6.775 -0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 447ebb74-4df3-4fc3-a41c-88d6277a42b1))
    (fp_line (start 6.775 -0.95) (end 0.775 -0.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 85c3ed47-7959-4de9-82f8-0dc27b52c5ee))
    (fp_line (start 6.775 0.95) (end 6.775 1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 014b4b8b-1ff3-47cf-b9e9-9f34635a24c8))
    (fp_line (start 6.775 1.59) (end 0.775 1.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48ebd49c-7067-4480-9e8c-b995573cf0fc))
    (fp_line (start 6.775 3.49) (end 6.775 4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp df76bd8a-b6ec-4d06-9e4c-538b48d9fe56))
    (fp_line (start 6.775 4.13) (end 0.775 4.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab11242d-b3bc-4cff-ac6f-14025505c5d4))
    (pad "" smd rect (at 3.895 -3.81) (size 6 0.76) (layers "F.SilkS") (tstamp ecd9dafa-9e1b-4a76-a561-8785717a9bf2))
    (pad "1" smd rect (at -5.525 -3.81) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (tstamp a5fe2370-de92-4d02-b57e-3f317f696a80))
    (pad "2" smd rect (at -5.525 -1.27) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (tstamp b13dad14-5f75-47b8-8828-be2875448800))
    (pad "3" smd rect (at -5.525 1.27) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/Yoman/A") (pinfunction "Pin_3") (pintype "passive") (tstamp 587e96b8-2cb4-4427-89ee-8b005bf08487))
    (pad "4" smd rect (at -5.525 3.81) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/Yoman/B") (pinfunction "Pin_4") (pintype "passive") (tstamp afcb349a-37e4-44f6-a75a-93d5fea63d57))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89004xx_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-14_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp 6c3cdf57-c5a1-4807-897f-fd17b7eda9a4)
    (at 167.64 111.76)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "WillItBlend.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad operational amplifier")
    (property "ki_keywords" "quad opamp")
    (path "/5fdfc049-65c9-4c1c-97ac-872853abcae6")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bda6c175-697f-42bd-817c-9035a2c57679)
    )
    (fp_text value "Opamp_Quad" (at 3.81 17.57) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ddeb99f-9ff3-46de-8110-09bedcd057c8)
    )
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2dffcaee-362f-4d95-ab23-129e3b2fbb2c)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 16.57)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3f77187-e72b-4c74-91cb-08b490a6f7f3))
    (fp_line (start 1.56 16.57) (end 6.06 16.57)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 311ea4d6-5a6a-4a6a-a816-e15edd357238))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fd8154b6-11af-4437-a0fc-dc7eccd089e3))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp df566a87-3a98-4512-9a30-870a0c5ed5d9))
    (fp_line (start 6.06 16.57) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 68576735-ab19-486a-a6d3-6eb81f2fd9dd))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f623861-48cc-4aec-84ba-1a0bd0e913ba))
    (fp_line (start -1.45 -1.55) (end -1.45 16.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 03375021-52e0-442d-ad4d-f7d674a69b72))
    (fp_line (start -1.45 16.8) (end 9.1 16.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e733191a-f755-4759-a2b3-97e26faa29af))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea9e8d5d-57df-4ed6-9308-686d3d8a88a0))
    (fp_line (start 9.1 16.8) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f0d9ef8f-e92e-43e2-8ffa-7c4c4b5b2dc9))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 71223296-ff60-4647-939a-59a1232634ba))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b10b818-2387-4047-97aa-7093a46e3f60))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 080d659e-9799-47bd-a9a3-23079c12febb))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 416b7aa4-fbbc-4179-94bd-a803bdcd90ac))
    (fp_line (start 6.985 16.51) (end 0.635 16.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4efdc317-a234-4b09-a8ad-e541ee58bcb6))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "/Yoman/C") (pintype "output") (tstamp ddbeb314-8864-4bd5-8db2-e1e459f161fc))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/Yoman/B") (pinfunction "-") (pintype "input") (tstamp f64883a3-5953-4db8-8a0c-301e0bc59b2f))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/Yoman/A") (pinfunction "+") (pintype "input") (tstamp a5cb9a4d-8616-4f86-95d3-da46589ee335))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "V+") (pintype "power_in") (tstamp b731ddfa-6119-4c31-b01c-a8b07c7ebe87))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "/Yoman/C") (pinfunction "+") (pintype "input") (tstamp 1942a05a-d49c-4bbf-afbf-aae3f2540147))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/Yoman/B") (pinfunction "-") (pintype "input") (tstamp c3ce4c85-fd18-4125-b239-400f8986a9b1))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/Yoman1/C") (pintype "output") (tstamp da96c6bc-123c-427a-bde1-de9eeede30ac))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/Yoman2/C") (pintype "output") (tstamp 0616123d-b85c-4702-a22d-8266782110f5))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/Yoman/B") (pinfunction "-") (pintype "input") (tstamp 3ba08f6e-9858-40d8-a949-e8f9d4e7f0df))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/Yoman1/C") (pinfunction "+") (pintype "input") (tstamp 1bb5ef6b-828a-4889-b3c7-98c69b00f41e))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "V-") (pintype "power_in") (tstamp aa7c0428-7d91-4854-ae62-0ebe6b95dd7a))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/Yoman2/C") (pinfunction "+") (pintype "input") (tstamp 34e0c826-82b6-411a-8a03-afe93fbad4b8))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/Yoman/A") (pinfunction "-") (pintype "input") (tstamp 7150dd49-198e-4859-89e9-aaa91141d944))
    (pad "14" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/Yoman3/C") (pintype "output") (tstamp e73da2ac-637b-44d8-aea2-c7d20009d8c5))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x01_P2.00mm_Vertical" (layer "F.Cu")
    (tstamp 7626bf10-5357-4ff6-98ef-2b5801aaba14)
    (at 179.29 123.92)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (property "Sheetfile" "WillItBlend.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (path "/2db49c73-cf63-4b02-b1a6-b0a350786ad5")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.06) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 69eec72e-08fe-4b93-b79b-de2a6eff9b4e)
    )
    (fp_text value "Conn_01x01_Pin" (at 0 2.06) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a3f17c0a-99a3-4ff6-8af3-4f034b2dc378)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ae577a0-ee8a-455c-b9c7-d37c94f1090d)
    )
    (fp_line (start -1.06 -1.06) (end 0 -1.06)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a51dc96-a9fe-4b62-8af2-3601b08b575b))
    (fp_line (start -1.06 0) (end -1.06 -1.06)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6590bb55-f723-4994-9f9b-05212517fce1))
    (fp_line (start -1.06 1) (end -1.06 1.06)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e7208bd-018c-4d79-bc7c-84953a1c5247))
    (fp_line (start -1.06 1) (end 1.06 1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdba8490-eb3b-4d5c-8462-b5b9b8fbc953))
    (fp_line (start -1.06 1.06) (end 1.06 1.06)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 206f601d-e5c0-4a98-8c08-fdb02af22f04))
    (fp_line (start 1.06 1) (end 1.06 1.06)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f95dd9d8-6610-4f32-b4ea-fa90584eca55))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9bd23c8-1a6d-48a5-9b72-e2976d392a92))
    (fp_line (start -1.5 1.5) (end 1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b18896a6-958e-4aa7-ad18-7ddf70d7d892))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f9cea3f-2add-4d9e-8dbe-eb6af219da06))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cab93955-fbe5-4759-bf94-3a7659407eb8))
    (fp_line (start -1 -0.5) (end -0.5 -1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e2e5b78-29b7-4470-9d3a-ea46ff28829b))
    (fp_line (start -1 1) (end -1 -0.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afa5b725-415a-4850-95cc-4cca513fbe96))
    (fp_line (start -0.5 -1) (end 1 -1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab8ce8ae-52f2-47d1-be80-f6dcf49cc3e1))
    (fp_line (start 1 -1) (end 1 1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c404da89-bc20-4786-a1b3-d323bc83b07a))
    (fp_line (start 1 1) (end -1 1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d312f12-1ba6-4d1e-aee5-02307fc6b3af))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/Yoman3/C") (pinfunction "Pin_1") (pintype "passive") (tstamp 711cbb6d-43d6-49d9-b57e-942229285fd4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x01_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
