(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")

  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 123)
    (zones 0)
    (modules 167)
    (nets 41)
  )

  (page User 189.992 210.007)
  (title_block
    (title "Power load")
    (date 2019-05-23)
    (rev 1.1)
    (company "BK Development")
    (comment 1 "Jonatan Gezelius 2019")
  )

  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.25)
    (user_trace_width 5)
    (user_trace_width 8)
    (user_trace_width 10)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot/"))
  )

  (net 0 "")
  (net 1 "Net-(R1-Pad2)")
  (net 2 "Net-(R3-Pad2)")
  (net 3 "Net-(R5-Pad2)")
  (net 4 "Net-(R7-Pad2)")
  (net 5 "Net-(R10-Pad1)")
  (net 6 "Net-(R11-Pad2)")
  (net 7 "Net-(R13-Pad2)")
  (net 8 "Net-(R15-Pad2)")
  (net 9 "Net-(R17-Pad2)")
  (net 10 "Net-(R19-Pad2)")
  (net 11 "Net-(R21-Pad2)")
  (net 12 "Net-(R23-Pad2)")
  (net 13 "Net-(R25-Pad2)")
  (net 14 "Net-(R27-Pad2)")
  (net 15 "Net-(R29-Pad2)")
  (net 16 "Net-(R31-Pad2)")
  (net 17 "Net-(R33-Pad2)")
  (net 18 "Net-(R35-Pad2)")
  (net 19 "Net-(R37-Pad2)")
  (net 20 "Net-(R39-Pad2)")
  (net 21 "Net-(J3-Pad1)")
  (net 22 "Net-(J4-Pad1)")
  (net 23 "Net-(J5-Pad1)")
  (net 24 "Net-(J6-Pad1)")
  (net 25 "Net-(R41-Pad2)")
  (net 26 "Net-(R42-Pad2)")
  (net 27 "Net-(R44-Pad2)")
  (net 28 "Net-(R45-Pad2)")
  (net 29 "Net-(R47-Pad2)")
  (net 30 "Net-(R48-Pad2)")
  (net 31 "Net-(R50-Pad2)")
  (net 32 "Net-(R51-Pad2)")
  (net 33 "Net-(R53-Pad2)")
  (net 34 "Net-(R54-Pad2)")
  (net 35 "Net-(R56-Pad2)")
  (net 36 "Net-(R57-Pad2)")
  (net 37 "Net-(R59-Pad2)")
  (net 38 "Net-(R61-Pad2)")
  (net 39 /2ohmA)
  (net 40 /2ohmB)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class 2Ohm ""
    (clearance 1.5)
    (trace_width 8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /2ohmA)
    (add_net /2ohmB)
  )

  (net_class Power ""
    (clearance 1.5)
    (trace_width 5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R35-Pad2)")
    (add_net "Net-(R37-Pad2)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R41-Pad2)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(R44-Pad2)")
    (add_net "Net-(R45-Pad2)")
    (add_net "Net-(R47-Pad2)")
    (add_net "Net-(R48-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(R51-Pad2)")
    (add_net "Net-(R53-Pad2)")
    (add_net "Net-(R54-Pad2)")
    (add_net "Net-(R56-Pad2)")
    (add_net "Net-(R57-Pad2)")
    (add_net "Net-(R59-Pad2)")
    (add_net "Net-(R61-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE7181C)
    (at 120.1 147.8 180)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE71815)
    (at 102.1 147.8 180)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE7180E)
    (at 120.1 158 180)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE71807)
    (at 102.1 158 180)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module custom_footprint:MountingHole_2.5mm_Pad_nocrtyd (layer F.Cu) (tedit 5CE67F80) (tstamp 5CE71170)
    (at 56.9 156.8)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (path /5CE8328D)
    (attr virtual)
    (fp_text reference J8 (at 0 -3.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.5 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
  )

  (module custom_footprint:MountingHole_2.5mm_Pad_nocrtyd (layer F.Cu) (tedit 5CE67F80) (tstamp 5CE7040B)
    (at 57 144.4)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (path /5CE7AAE3)
    (attr virtual)
    (fp_text reference J9 (at 0 -3.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.5 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
  )

  (module custom_footprint:MountingHole_2.5mm_Pad_nocrtyd (layer F.Cu) (tedit 5CE67F80) (tstamp 5CE6847D)
    (at 57 94)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (path /5CE6E742)
    (attr virtual)
    (fp_text reference J7 (at 0 -3.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.5 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
  )

  (module custom_footprint:Fan_120mm (layer F.Cu) (tedit 5CE55560) (tstamp 5CE5DC51)
    (at 88.9 94.8)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fan_120mm (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 52.5 -52.5) (end 57.5 -52.5) (layer F.CrtYd) (width 0.12))
    (fp_circle (center 52.5 52.5) (end 57.5 52.5) (layer F.CrtYd) (width 0.12))
    (fp_circle (center -52.5 52.5) (end -47.5 52.5) (layer F.CrtYd) (width 0.12))
    (fp_circle (center -52.5 -52.5) (end -47.5 -52.5) (layer F.CrtYd) (width 0.12))
    (fp_line (start -60 60) (end -60 -60) (layer F.Fab) (width 0.12))
    (fp_line (start 60 60) (end -60 60) (layer F.Fab) (width 0.12))
    (fp_line (start 60 -60) (end 60 60) (layer F.Fab) (width 0.12))
    (fp_line (start -60 -60) (end 60 -60) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 52.5 -52.5 270) (size 5 5) (drill 4.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 52.5 52.5 180) (size 5 5) (drill 4.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -52.5 52.5 90) (size 5 5) (drill 4.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -52.5 -52.5) (size 5 5) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE67061)
    (at 159.3 122.6 90)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE6705A)
    (at 159.3 140.6 90)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE67053)
    (at 169.5 122.6 90)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE6704C)
    (at 169.5 140.6 90)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66FBA)
    (at 155.9 60.1)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66FB3)
    (at 168.3 60.1)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F63)
    (at 155.9 46.8)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F63)
    (at 168.3 46.8)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F63)
    (at 148.3 21)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F63)
    (at 148.3 32.2)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F63)
    (at 166.3 32.2)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CE66F31)
    (at 166.3 21)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CE602B5)
    (at 104.5 25.1 270)
    (path /5CDC1336)
    (fp_text reference J6 (at 0 -4 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad1)"))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CE60210)
    (at 132.7 25.1 270)
    (path /5CDC0510)
    (fp_text reference J5 (at 0 -4 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad1)"))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CD9EEC4)
    (at 164.4 89.2 180)
    (path /5CDC1A5E)
    (fp_text reference J4 (at 0 -4 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CE60332)
    (at 164.4 75)
    (path /5CDC144C)
    (fp_text reference J3 (at 0 -4) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CE69B27)
    (at 57 20.4)
    (path /5CD6A227)
    (fp_text reference J2 (at 0 -4) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
  )

  (module custom_footprint:cable_solder_2.5mm^2 (layer F.Cu) (tedit 5CE54BB2) (tstamp 5CE5EC08)
    (at 57 33.7)
    (path /5CD692B4)
    (fp_text reference J1 (at 0 -4) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0.25 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer B.Cu) (width 0.1))
    (fp_poly (pts (xy -5 -5) (xy 5 -5) (xy 5 5) (xy -5 5)) (layer F.Cu) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 2.5) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE63873)
    (at 146.7 82)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60D4F)
    (at 123.1 35)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60D48)
    (at 113.1 35)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 123.1 45)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 113.1 45)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 46 35.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 46 45.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 67 35.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 77 35.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 77 45.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 67 45.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 141.8 57.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 141.8 67.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60CAB)
    (at 131.8 67.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C4A)
    (at 101.9 67.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C43)
    (at 111.9 67.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C3C)
    (at 121.9 67.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C4A)
    (at 116.7 82)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C43)
    (at 126.7 82)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60C3C)
    (at 136.7 82)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BAE)
    (at 110.8 141.6)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA7)
    (at 127.5 141.6)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BAE)
    (at 110.8 132.1)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA7)
    (at 127.5 132.1)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA0)
    (at 144.4 132.1)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BAE)
    (at 110.8 122.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA7)
    (at 127.5 122.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA0)
    (at 144.4 122.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BAE)
    (at 110.8 113)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA7)
    (at 127.5 113)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA0)
    (at 144.4 113)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BAE)
    (at 110.8 103.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA7)
    (at 127.5 103.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60BA0)
    (at 144.4 103.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 110.8 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 127.5 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 144.4 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 141.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 141.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 141.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 141.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 132)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 132)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 132)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 132)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 122.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 122.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 122.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 122.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 112.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 112.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 112.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 112.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 103.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 103.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 103.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 103.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6070D)
    (at 31.1 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60706)
    (at 47 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606FF)
    (at 67.1 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE606F8)
    (at 83 93.9)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60613)
    (at 31.1 84.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6060C)
    (at 47 84.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60605)
    (at 67.1 84.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE605FE)
    (at 83 84.4)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60613)
    (at 31.1 74.8)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6060C)
    (at 47 74.8)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60605)
    (at 67.1 74.8)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE605FE)
    (at 83 74.8)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60552)
    (at 31.1 65.3)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6054B)
    (at 47 65.3)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE60544)
    (at 67.1 65.3)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE6053D)
    (at 83 65.3)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CDEE9CF)
    (at 110.72 55.979721)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CDEE9C8)
    (at 126.6 55.979721)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE604C3)
    (at 82.9 56)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE604BC)
    (at 67 56)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE604B5)
    (at 47.1 56)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:VentilationHole_3.5mm (layer F.Cu) (tedit 5CE54AE2) (tstamp 5CE604AE)
    (at 31 56)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VentilationHole_3.5mm (at 0 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.8 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD050CD)
    (at 48 117.821106 180)
    (path /5CD0583D)
    (fp_text reference R15 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CDEBCA7)
    (at 30 117.821106 180)
    (path /5CD0E3A5)
    (fp_text reference R16 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(R15-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD050FB)
    (at 48 127.36055 180)
    (path /5CCFE912)
    (fp_text reference R17 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05112)
    (at 30 127.36055 180)
    (path /5CD0E34B)
    (fp_text reference R18 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(R17-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D278)
    (at 48 51.4 180)
    (path /5CD05813)
    (fp_text reference R1 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D503)
    (at 30 51.404721 180)
    (path /5CD0E37B)
    (fp_text reference R2 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A52F)
    (at 48 60.584442 180)
    (path /5CD05819)
    (fp_text reference R3 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD07DF7)
    (at 30 60.584442 180)
    (path /5CD0E381)
    (fp_text reference R4 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(R3-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD04FE7)
    (at 48 70.123886 180)
    (path /5CD0581F)
    (fp_text reference R5 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD04FFE)
    (at 30 70.123886 180)
    (path /5CD0E387)
    (fp_text reference R6 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(R5-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05015)
    (at 48 79.66333 180)
    (path /5CD05825)
    (fp_text reference R7 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0502C)
    (at 30 79.66333 180)
    (path /5CD0E38D)
    (fp_text reference R8 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(R7-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05043)
    (at 48 89.202774 180)
    (path /5CD0582B)
    (fp_text reference R9 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0505A)
    (at 30 89.202774 180)
    (path /5CD0E393)
    (fp_text reference R10 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05071)
    (at 48 98.742218 180)
    (path /5CD05831)
    (fp_text reference R11 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05088)
    (at 30 98.742218 180)
    (path /5CD0E399)
    (fp_text reference R12 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(R11-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0509F)
    (at 48 108.281662 180)
    (path /5CD05837)
    (fp_text reference R13 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD050B6)
    (at 30 108.281662 180)
    (path /5CD0E39F)
    (fp_text reference R14 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(R13-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05129)
    (at 48 136.9 180)
    (path /5CCFEE45)
    (fp_text reference R19 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 10 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C3CF)
    (at 30 136.9 180)
    (path /5CD0E351)
    (fp_text reference R20 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 10 "Net-(R19-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BAA7)
    (at 109.6 60.584442 180)
    (path /5CDA7F18)
    (fp_text reference R62 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 38 "Net-(R61-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BA80)
    (at 127.6 60.584442 180)
    (path /5CDA796A)
    (fp_text reference R61 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 38 "Net-(R61-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D131)
    (at 109.6 51.4 180)
    (path /5CDA7BB2)
    (fp_text reference R60 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 37 "Net-(R59-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D42F)
    (at 127.6 51.4 180)
    (path /5CDA70BD)
    (fp_text reference R59 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 37 "Net-(R59-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D8F6)
    (at 145.6 89.202774)
    (path /5CDB5737)
    (fp_text reference R58 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 36 "Net-(R57-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D872)
    (at 127.6 89.202774)
    (path /5CDB5731)
    (fp_text reference R57 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 36 "Net-(R57-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 35 "Net-(R56-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C0EA)
    (at 109.6 89.202774)
    (path /5CDB572B)
    (fp_text reference R56 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 35 "Net-(R56-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C0C3)
    (at 145.6 98.742218)
    (path /5CDB5723)
    (fp_text reference R55 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 34 "Net-(R54-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C09C)
    (at 127.6 98.742218)
    (path /5CDB571D)
    (fp_text reference R54 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 34 "Net-(R54-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 33 "Net-(R53-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C075)
    (at 109.6 98.742218)
    (path /5CDB5717)
    (fp_text reference R53 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 33 "Net-(R53-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C04E)
    (at 145.6 108.281662)
    (path /5CDAE460)
    (fp_text reference R52 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 32 "Net-(R51-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C027)
    (at 127.6 108.281662)
    (path /5CDAE45A)
    (fp_text reference R51 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 32 "Net-(R51-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 31 "Net-(R50-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5C000)
    (at 109.6 108.281662)
    (path /5CDAE454)
    (fp_text reference R50 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 31 "Net-(R50-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BFD9)
    (at 145.6 117.821106)
    (path /5CDAE44C)
    (fp_text reference R49 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 30 "Net-(R48-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BFB2)
    (at 127.6 117.821106)
    (path /5CDAE446)
    (fp_text reference R48 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 30 "Net-(R48-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 29 "Net-(R47-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BF8B)
    (at 109.6 117.821106)
    (path /5CDAE440)
    (fp_text reference R47 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 29 "Net-(R47-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BF64)
    (at 145.6 127.36055)
    (path /5CDAA569)
    (fp_text reference R46 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 28 "Net-(R45-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BF3D)
    (at 127.6 127.36055)
    (path /5CDAA563)
    (fp_text reference R45 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 28 "Net-(R45-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 27 "Net-(R44-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BF16)
    (at 109.6 127.36055)
    (path /5CDAA55D)
    (fp_text reference R44 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 27 "Net-(R44-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BEEF)
    (at 145.6 136.9)
    (path /5CDA8BA6)
    (fp_text reference R43 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 26 "Net-(R42-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BEC8)
    (at 127.6 136.9)
    (path /5CDA8A1F)
    (fp_text reference R42 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 26 "Net-(R42-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 25 "Net-(R41-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5BEA1)
    (at 109.6 136.9)
    (path /5CDA811D)
    (fp_text reference R41 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 25 "Net-(R41-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A1FC)
    (at 84 136.9)
    (path /5CD0E3BD)
    (fp_text reference R40 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 20 "Net-(R39-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD052F5)
    (at 66 136.9)
    (path /5CD06A9D)
    (fp_text reference R39 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 20 "Net-(R39-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A23E)
    (at 84 127.36055)
    (path /5CD0E3B7)
    (fp_text reference R38 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 19 "Net-(R37-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD052C7)
    (at 66 127.36055)
    (path /5CD06A97)
    (fp_text reference R37 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 19 "Net-(R37-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A280)
    (at 84 117.821106)
    (path /5CD0E3B1)
    (fp_text reference R36 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 18 "Net-(R35-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD05299)
    (at 66 117.821106)
    (path /5CD06A91)
    (fp_text reference R35 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 18 "Net-(R35-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A2C2)
    (at 84 108.281662)
    (path /5CD0E3AB)
    (fp_text reference R34 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 17 "Net-(R33-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0526B)
    (at 66 108.281662)
    (path /5CD06A8B)
    (fp_text reference R33 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 17 "Net-(R33-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A304)
    (at 84 98.742218)
    (path /5CD0E375)
    (fp_text reference R32 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 16 "Net-(R31-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0523D)
    (at 66 98.742218)
    (path /5CD02DF3)
    (fp_text reference R31 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 16 "Net-(R31-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A346)
    (at 84 89.202774)
    (path /5CD0E36F)
    (fp_text reference R30 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 15 "Net-(R29-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0520F)
    (at 66 89.202774)
    (path /5CD02DED)
    (fp_text reference R29 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 15 "Net-(R29-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A388)
    (at 84 79.66333)
    (path /5CD0E369)
    (fp_text reference R28 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 14 "Net-(R27-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD051E1)
    (at 66 79.66333)
    (path /5CD02DE7)
    (fp_text reference R27 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 14 "Net-(R27-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A40C)
    (at 84 70.123886)
    (path /5CD0E363)
    (fp_text reference R26 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 13 "Net-(R25-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD051B3)
    (at 66 70.123886)
    (path /5CD02DE1)
    (fp_text reference R25 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 13 "Net-(R25-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CD0A44E)
    (at 84 60.584442)
    (path /5CD0E35D)
    (fp_text reference R24 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 12 "Net-(R23-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CDED1A1)
    (at 66 60.584442)
    (path /5CD00D29)
    (fp_text reference R23 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 12 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D4C1)
    (at 84 51.4)
    (path /5CD0E357)
    (fp_text reference R22 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(R21-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 40 /2ohmB))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100_round_holes locked (layer F.Cu) (tedit 5CDE59AF) (tstamp 5CE5D381)
    (at 66 51.4)
    (path /5CD00D23)
    (fp_text reference R21 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at -5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 39 /2ohmA))
    (pad 2 thru_hole circle (at 5.08 0) (size 5 5) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "B\n\n2Ω\n\nA" (at 51.5 151.2) (layer F.SilkS) (tstamp 5CE753A9)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_poly (pts (xy 50.5 49) (xy 52 49) (xy 52 30.5) (xy 62 30.5) (xy 62 49) (xy 63.5 49) (xy 63.5 139.5) (xy 61.5 146.5) (xy 52.5 146.5) (xy 50.5 139.5)) (layer B.Mask) (width 0.1))
  (gr_poly (pts (xy 17.5 30) (xy 17 140) (xy 19.5 140.25) (xy 19.5 154.75) (xy 25.5 161) (xy 88 161) (xy 94.5 155) (xy 94.5 140) (xy 96.5 140) (xy 96.5 33.5) (xy 78.5 15.5) (xy 32.5 15.5) (xy 17.5 30) (xy 27.5 34.5) (xy 36.5 25) (xy 74 25) (xy 86.5 38) (xy 86.5 151) (xy 84.5 153) (xy 29 153) (xy 27.5 151.5) (xy 27.5 34.5)) (layer B.Mask) (width 0.1))
  (gr_text "2Ω B" (at 57.1 100.4 90) (layer F.SilkS) (tstamp 5CE718E1)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text "Jonatan Gezelius 2019" (at 146.8 156.8) (layer F.SilkS) (tstamp 5CE55617)
    (effects (font (size 1.5 1.5) (thickness 0.2)) (justify left))
  )
  (gr_text "BK Services AB" (at 146.7 158.9) (layer F.SilkS) (tstamp 5CE55616)
    (effects (font (size 1.5 1.5) (thickness 0.2)) (justify left))
  )
  (gr_text "Konstlast v1.1" (at 146.7 160.9) (layer F.SilkS) (tstamp 5CE55615)
    (effects (font (size 1.5 1.5) (thickness 0.2)) (justify left))
  )
  (gr_text B (at 164.5 95.6) (layer F.SilkS) (tstamp 5CE610DD)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text A (at 164.8 68.8) (layer F.SilkS) (tstamp 5CE610DD)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text 10Ω (at 164.5 82.2) (layer F.SilkS) (tstamp 5CDF3832)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text "A\n\n2Ω\n\nB" (at 51 27.1) (layer F.SilkS) (tstamp 5CE5DBA9)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text "A 50Ω B" (at 119.3 22.6) (layer F.SilkS)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_line (start 14.4 13.9) (end 174.4 13.9) (layer Edge.Cuts) (width 0.05) (tstamp 5CE5F7BE))
  (gr_line (start 14.4 163.9) (end 14.4 13.9) (layer Edge.Cuts) (width 0.05) (tstamp 5CE5F7BB))
  (gr_line (start 174.4 163.9) (end 14.4 163.9) (layer Edge.Cuts) (width 0.05) (tstamp 5CE5F7B8))
  (gr_line (start 174.4 13.9) (end 174.4 163.9) (layer Edge.Cuts) (width 0.05) (tstamp 5CE5F7B5))

  (segment (start 42.915279 51.404721) (end 42.92 51.4) (width 5) (layer F.Cu) (net 1))
  (segment (start 35.08 51.404721) (end 42.915279 51.404721) (width 5) (layer F.Cu) (net 1))
  (segment (start 35.084721 51.4) (end 35.08 51.404721) (width 5) (layer B.Cu) (net 1))
  (segment (start 42.92 51.4) (end 35.084721 51.4) (width 5) (layer B.Cu) (net 1))
  (segment (start 42.92 60.584442) (end 35.08 60.584442) (width 5) (layer F.Cu) (net 2))
  (segment (start 35.08 60.584442) (end 42.92 60.584442) (width 5) (layer B.Cu) (net 2))
  (segment (start 35.08 70.123886) (end 42.92 70.123886) (width 5) (layer F.Cu) (net 3))
  (segment (start 42.92 70.123886) (end 35.08 70.123886) (width 5) (layer B.Cu) (net 3))
  (segment (start 42.92 79.66333) (end 35.08 79.66333) (width 5) (layer F.Cu) (net 4))
  (segment (start 35.08 79.66333) (end 42.92 79.66333) (width 5) (layer B.Cu) (net 4))
  (segment (start 42.92 89.202774) (end 35.08 89.202774) (width 5) (layer F.Cu) (net 5))
  (segment (start 42.92 89.202774) (end 35.08 89.202774) (width 5) (layer B.Cu) (net 5))
  (segment (start 42.92 98.742218) (end 35.08 98.742218) (width 5) (layer F.Cu) (net 6))
  (segment (start 35.08 98.742218) (end 42.92 98.742218) (width 5) (layer B.Cu) (net 6))
  (segment (start 42.92 108.281662) (end 35.08 108.281662) (width 5) (layer F.Cu) (net 7))
  (segment (start 42.92 108.281662) (end 35.08 108.281662) (width 5) (layer B.Cu) (net 7))
  (segment (start 42.92 117.821106) (end 35.08 117.821106) (width 5) (layer F.Cu) (net 8))
  (segment (start 35.08 117.821106) (end 42.92 117.821106) (width 5) (layer B.Cu) (net 8))
  (segment (start 42.92 127.36055) (end 35.08 127.36055) (width 5) (layer F.Cu) (net 9))
  (segment (start 42.92 127.36055) (end 35.08 127.36055) (width 5) (layer B.Cu) (net 9))
  (segment (start 35.08 136.9) (end 42.92 136.9) (width 5) (layer F.Cu) (net 10))
  (segment (start 35.08 136.9) (end 42.92 136.9) (width 5) (layer B.Cu) (net 10))
  (segment (start 78.92 51.4) (end 71.08 51.4) (width 5) (layer F.Cu) (net 11))
  (segment (start 71.08 51.4) (end 78.92 51.4) (width 5) (layer B.Cu) (net 11))
  (segment (start 71.08 60.584442) (end 78.92 60.584442) (width 5) (layer F.Cu) (net 12))
  (segment (start 78.92 60.584442) (end 71.08 60.584442) (width 5) (layer B.Cu) (net 12))
  (segment (start 78.92 70.123886) (end 71.08 70.123886) (width 5) (layer F.Cu) (net 13))
  (segment (start 71.08 70.123886) (end 78.92 70.123886) (width 5) (layer B.Cu) (net 13))
  (segment (start 71.08 79.66333) (end 78.92 79.66333) (width 5) (layer F.Cu) (net 14))
  (segment (start 78.92 79.66333) (end 71.08 79.66333) (width 5) (layer B.Cu) (net 14))
  (segment (start 78.92 89.202774) (end 71.08 89.202774) (width 5) (layer F.Cu) (net 15))
  (segment (start 71.08 89.202774) (end 78.92 89.202774) (width 5) (layer B.Cu) (net 15))
  (segment (start 71.08 98.742218) (end 78.92 98.742218) (width 5) (layer F.Cu) (net 16))
  (segment (start 78.92 98.742218) (end 71.08 98.742218) (width 5) (layer B.Cu) (net 16))
  (segment (start 78.92 108.281662) (end 71.08 108.281662) (width 5) (layer F.Cu) (net 17))
  (segment (start 71.08 108.281662) (end 78.92 108.281662) (width 5) (layer B.Cu) (net 17))
  (segment (start 71.08 117.821106) (end 78.92 117.821106) (width 5) (layer F.Cu) (net 18))
  (segment (start 78.92 117.821106) (end 71.08 117.821106) (width 5) (layer B.Cu) (net 18))
  (segment (start 78.92 127.36055) (end 71.08 127.36055) (width 5) (layer F.Cu) (net 19))
  (segment (start 71.08 127.36055) (end 78.92 127.36055) (width 5) (layer B.Cu) (net 19))
  (segment (start 71.08 136.9) (end 78.92 136.9) (width 5) (layer F.Cu) (net 20))
  (segment (start 78.92 136.9) (end 71.08 136.9) (width 5) (layer B.Cu) (net 20))
  (segment (start 166.9 75) (end 161.9 75) (width 5) (layer F.Cu) (net 21))
  (segment (start 104.52 89.202774) (end 104.52 136.9) (width 5) (layer F.Cu) (net 21))
  (segment (start 104.52 84.18) (end 104.52 89.202774) (width 5) (layer F.Cu) (net 21))
  (segment (start 161.9 75) (end 113.7 75) (width 5) (layer F.Cu) (net 21))
  (segment (start 113.7 75) (end 104.52 84.18) (width 5) (layer F.Cu) (net 21))
  (segment (start 104.52 136.9) (end 104.52 89.202774) (width 5) (layer B.Cu) (net 21))
  (segment (start 113.7 75) (end 166.9 75) (width 5) (layer B.Cu) (net 21))
  (segment (start 104.52 89.202774) (end 104.52 84.18) (width 5) (layer B.Cu) (net 21))
  (segment (start 104.52 84.18) (end 113.7 75) (width 5) (layer B.Cu) (net 21))
  (segment (start 150.682774 89.2) (end 150.68 89.202774) (width 5) (layer F.Cu) (net 22))
  (segment (start 161.9 89.2) (end 150.682774 89.2) (width 5) (layer F.Cu) (net 22))
  (segment (start 166.9 89.2) (end 161.9 89.2) (width 5) (layer F.Cu) (net 22))
  (segment (start 150.68 89.202774) (end 150.68 136.9) (width 5) (layer F.Cu) (net 22))
  (segment (start 150.68 136.9) (end 150.68 89.202774) (width 5) (layer B.Cu) (net 22))
  (segment (start 161.897226 89.202774) (end 161.9 89.2) (width 5) (layer B.Cu) (net 22))
  (segment (start 150.68 89.202774) (end 161.897226 89.202774) (width 5) (layer B.Cu) (net 22))
  (segment (start 161.9 89.2) (end 166.9 89.2) (width 5) (layer B.Cu) (net 22))
  (segment (start 132.68 51.4) (end 132.68 60.584442) (width 5) (layer F.Cu) (net 23))
  (segment (start 132.7 22.6) (end 132.7 27.6) (width 5) (layer F.Cu) (net 23))
  (segment (start 132.7 51.38) (end 132.68 51.4) (width 5) (layer F.Cu) (net 23))
  (segment (start 132.7 27.6) (end 132.7 51.38) (width 5) (layer F.Cu) (net 23))
  (segment (start 132.68 22.62) (end 132.7 22.6) (width 5) (layer B.Cu) (net 23))
  (segment (start 132.68 60.584442) (end 132.68 22.62) (width 5) (layer B.Cu) (net 23))
  (segment (start 104.52 60.584442) (end 104.52 51.4) (width 5) (layer F.Cu) (net 24))
  (segment (start 104.52 27.62) (end 104.5 27.6) (width 5) (layer F.Cu) (net 24))
  (segment (start 104.52 51.4) (end 104.52 27.62) (width 5) (layer F.Cu) (net 24))
  (segment (start 104.5 22.6) (end 104.5 27.6) (width 5) (layer F.Cu) (net 24))
  (segment (start 104.52 60.584442) (end 104.52 51.4) (width 5) (layer B.Cu) (net 24))
  (segment (start 104.52 27.62) (end 104.5 27.6) (width 5) (layer B.Cu) (net 24))
  (segment (start 104.52 51.4) (end 104.52 27.62) (width 5) (layer B.Cu) (net 24))
  (segment (start 122.52 136.9) (end 114.68 136.9) (width 5) (layer F.Cu) (net 25))
  (segment (start 114.68 136.9) (end 122.52 136.9) (width 5) (layer B.Cu) (net 25))
  (segment (start 132.68 136.9) (end 140.52 136.9) (width 5) (layer F.Cu) (net 26))
  (segment (start 132.68 136.9) (end 140.52 136.9) (width 5) (layer B.Cu) (net 26))
  (segment (start 114.68 127.36055) (end 122.52 127.36055) (width 5) (layer F.Cu) (net 27))
  (segment (start 122.52 127.36055) (end 114.68 127.36055) (width 5) (layer B.Cu) (net 27))
  (segment (start 140.52 127.36055) (end 132.68 127.36055) (width 5) (layer F.Cu) (net 28))
  (segment (start 140.52 127.36055) (end 132.68 127.36055) (width 5) (layer B.Cu) (net 28))
  (segment (start 122.52 117.821106) (end 114.68 117.821106) (width 5) (layer F.Cu) (net 29))
  (segment (start 114.68 117.821106) (end 122.52 117.821106) (width 5) (layer B.Cu) (net 29))
  (segment (start 132.68 117.821106) (end 140.52 117.821106) (width 5) (layer F.Cu) (net 30))
  (segment (start 132.68 117.821106) (end 140.52 117.821106) (width 5) (layer B.Cu) (net 30))
  (segment (start 114.68 108.281662) (end 122.52 108.281662) (width 5) (layer F.Cu) (net 31))
  (segment (start 122.52 108.281662) (end 114.68 108.281662) (width 5) (layer B.Cu) (net 31))
  (segment (start 140.52 108.281662) (end 132.68 108.281662) (width 5) (layer F.Cu) (net 32))
  (segment (start 140.52 108.281662) (end 132.68 108.281662) (width 5) (layer B.Cu) (net 32))
  (segment (start 122.52 98.742218) (end 114.68 98.742218) (width 5) (layer F.Cu) (net 33))
  (segment (start 114.68 98.742218) (end 122.52 98.742218) (width 5) (layer B.Cu) (net 33))
  (segment (start 140.52 98.742218) (end 132.68 98.742218) (width 5) (layer F.Cu) (net 34))
  (segment (start 132.68 98.742218) (end 140.52 98.742218) (width 5) (layer B.Cu) (net 34))
  (segment (start 114.68 89.202774) (end 122.52 89.202774) (width 5) (layer F.Cu) (net 35))
  (segment (start 122.52 89.202774) (end 114.68 89.202774) (width 5) (layer B.Cu) (net 35))
  (segment (start 132.68 89.202774) (end 140.52 89.202774) (width 5) (layer F.Cu) (net 36))
  (segment (start 140.52 89.202774) (end 132.68 89.202774) (width 5) (layer B.Cu) (net 36))
  (segment (start 114.68 51.4) (end 122.52 51.4) (width 5) (layer F.Cu) (net 37))
  (segment (start 114.68 51.4) (end 122.52 51.4) (width 5) (layer B.Cu) (net 37))
  (segment (start 122.52 60.584442) (end 114.68 60.584442) (width 5) (layer F.Cu) (net 38))
  (segment (start 122.52 60.584442) (end 114.68 60.584442) (width 5) (layer B.Cu) (net 38))
  (segment (start 57 34.7) (end 57 52) (width 10) (layer B.Cu) (net 39) (tstamp 5CE5F845))
  (segment (start 57 34.7) (end 57 52) (width 10) (layer F.Cu) (net 39) (tstamp 5CE5EBED))
  (segment (start 22.5 51.4) (end 22.5 32.2) (width 10) (layer B.Cu) (net 40) (tstamp 5CE66C26))
  (segment (start 23.5 136.88) (end 23.5 153.2) (width 8) (layer F.Cu) (net 40) (tstamp 5CE5EB33))
  (segment (start 23.5 153.2) (end 27.100001 156.800001) (width 8) (layer F.Cu) (net 40) (tstamp 5CE5EB34))
  (segment (start 27.100001 156.800001) (end 86.599999 156.800001) (width 8) (layer F.Cu) (net 40) (tstamp 5CE5EB35))
  (segment (start 86.599999 156.800001) (end 90.5 152.9) (width 8) (layer F.Cu) (net 40) (tstamp 5CE5EB36))
  (segment (start 90.5 152.9) (end 90.5 136.88) (width 8) (layer F.Cu) (net 40) (tstamp 5CE5EB37))
  (segment (start 90.5 152.9) (end 90.5 136.88) (width 8) (layer B.Cu) (net 40))
  (segment (start 86.599999 156.800001) (end 90.5 152.9) (width 8) (layer B.Cu) (net 40))
  (segment (start 27.100001 156.800001) (end 86.599999 156.800001) (width 8) (layer B.Cu) (net 40))
  (segment (start 23.5 136.88) (end 23.5 153.2) (width 8) (layer B.Cu) (net 40))
  (segment (start 23.5 153.2) (end 27.100001 156.800001) (width 8) (layer B.Cu) (net 40))
  (segment (start 91.5 35.88) (end 91.5 51.4) (width 10) (layer F.Cu) (net 40))
  (segment (start 76.04501 20.42501) (end 91.5 35.88) (width 10) (layer F.Cu) (net 40))
  (segment (start 34.27499 20.42501) (end 76.04501 20.42501) (width 10) (layer F.Cu) (net 40))
  (segment (start 22.5 51.4) (end 22.5 32.2) (width 10) (layer F.Cu) (net 40))
  (segment (start 22.5 32.2) (end 34.27499 20.42501) (width 10) (layer F.Cu) (net 40))
  (segment (start 91.5 35.88) (end 91.5 51.4) (width 10) (layer B.Cu) (net 40))
  (segment (start 76.04501 20.42501) (end 91.5 35.88) (width 10) (layer B.Cu) (net 40))
  (segment (start 34.27499 20.42501) (end 76.04501 20.42501) (width 10) (layer B.Cu) (net 40))
  (segment (start 22.5 36.775279) (end 22.5 32.2) (width 10) (layer B.Cu) (net 40))
  (segment (start 22.5 32.2) (end 34.27499 20.42501) (width 10) (layer B.Cu) (net 40))

  (zone (net 39) (net_name /2ohmA) (layer F.Cu) (tstamp 5CE73D94) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.6 139.4) (xy 53 148.9) (xy 61 148.9) (xy 63.4 139.4) (xy 63.4 48.9)
        (xy 50.6 48.9)
      )
    )
    (filled_polygon
      (pts
        (xy 63.273 139.384208) (xy 60.901095 148.773) (xy 53.098905 148.773) (xy 50.727 139.384208) (xy 50.727 49.027)
        (xy 63.273 49.027)
      )
    )
  )
  (zone (net 39) (net_name /2ohmA) (layer B.Cu) (tstamp 5CE73D91) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.6 139.4) (xy 53 148.9) (xy 61.1 148.9) (xy 63.4 139.4) (xy 63.4 48.9)
        (xy 50.6 48.9)
      )
    )
    (filled_polygon
      (pts
        (xy 63.273 139.384845) (xy 61.000078 148.773) (xy 53.098905 148.773) (xy 50.727 139.384208) (xy 50.727 49.027)
        (xy 63.273 49.027)
      )
    )
  )
  (zone (net 40) (net_name /2ohmB) (layer B.Cu) (tstamp 5CE73D8E) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.5 48.8) (xy 96.5 48.8) (xy 96.5 139.8) (xy 86.5 139.8)
      )
    )
    (filled_polygon
      (pts
        (xy 96.373 139.673) (xy 86.627 139.673) (xy 86.627 48.927) (xy 96.373 48.927)
      )
    )
  )
  (zone (net 40) (net_name /2ohmB) (layer B.Cu) (tstamp 5CE73D8B) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.5 48.7) (xy 17.5 48.7) (xy 17.5 139.7) (xy 27.5 139.7)
      )
    )
    (filled_polygon
      (pts
        (xy 27.373 139.573) (xy 17.627 139.573) (xy 17.627 48.827) (xy 27.373 48.827)
      )
    )
  )
  (zone (net 40) (net_name /2ohmB) (layer F.Cu) (tstamp 5CE73D88) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.5 48.8) (xy 96.5 48.8) (xy 96.5 139.8) (xy 86.5 139.8)
      )
    )
    (filled_polygon
      (pts
        (xy 96.373 139.673) (xy 86.627 139.673) (xy 86.627 48.927) (xy 96.373 48.927)
      )
    )
  )
  (zone (net 40) (net_name /2ohmB) (layer F.Cu) (tstamp 5CE73D85) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.5 48.7) (xy 17.5 48.7) (xy 17.5 139.7) (xy 27.5 139.7)
      )
    )
    (filled_polygon
      (pts
        (xy 27.373 139.573) (xy 17.627 139.573) (xy 17.627 48.827) (xy 27.373 48.827)
      )
    )
  )
)
