(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 78)
    (zones 0)
    (modules 73)
    (nets 41)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(R1-Pad2)")
  (net 4 "Net-(R3-Pad2)")
  (net 5 "Net-(R5-Pad2)")
  (net 6 "Net-(R7-Pad2)")
  (net 7 "Net-(R10-Pad1)")
  (net 8 "Net-(R11-Pad2)")
  (net 9 "Net-(R13-Pad2)")
  (net 10 "Net-(R15-Pad2)")
  (net 11 "Net-(R17-Pad2)")
  (net 12 "Net-(R19-Pad2)")
  (net 13 "Net-(R21-Pad2)")
  (net 14 "Net-(R23-Pad2)")
  (net 15 "Net-(R25-Pad2)")
  (net 16 "Net-(R27-Pad2)")
  (net 17 "Net-(R29-Pad2)")
  (net 18 "Net-(R31-Pad2)")
  (net 19 "Net-(R33-Pad2)")
  (net 20 "Net-(R35-Pad2)")
  (net 21 "Net-(R37-Pad2)")
  (net 22 "Net-(R39-Pad2)")
  (net 23 "Net-(J3-Pad1)")
  (net 24 "Net-(J4-Pad1)")
  (net 25 "Net-(J5-Pad1)")
  (net 26 "Net-(J6-Pad1)")
  (net 27 "Net-(R41-Pad2)")
  (net 28 "Net-(R42-Pad2)")
  (net 29 "Net-(R44-Pad2)")
  (net 30 "Net-(R45-Pad2)")
  (net 31 "Net-(R47-Pad2)")
  (net 32 "Net-(R48-Pad2)")
  (net 33 "Net-(R50-Pad2)")
  (net 34 "Net-(R51-Pad2)")
  (net 35 "Net-(R53-Pad2)")
  (net 36 "Net-(R54-Pad2)")
  (net 37 "Net-(R56-Pad2)")
  (net 38 "Net-(R57-Pad2)")
  (net 39 "Net-(R59-Pad2)")
  (net 40 "Net-(R61-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class Power ""
    (clearance 3)
    (trace_width 5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R35-Pad2)")
    (add_net "Net-(R37-Pad2)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R41-Pad2)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(R44-Pad2)")
    (add_net "Net-(R45-Pad2)")
    (add_net "Net-(R47-Pad2)")
    (add_net "Net-(R48-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(R51-Pad2)")
    (add_net "Net-(R53-Pad2)")
    (add_net "Net-(R54-Pad2)")
    (add_net "Net-(R56-Pad2)")
    (add_net "Net-(R57-Pad2)")
    (add_net "Net-(R59-Pad2)")
    (add_net "Net-(R61-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )

  (module custom_footprint:Fan_92mm locked (layer F.Cu) (tedit 5CD96DDC) (tstamp 5CDA4467)
    (at 127 90.25)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fan_92mm (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 41.25 -41.25) (end 41.25 -37.25) (layer F.CrtYd) (width 0.12))
    (fp_circle (center 41.25 41.25) (end 37.25 41.25) (layer F.CrtYd) (width 0.12))
    (fp_circle (center -41.25 41.25) (end -41.25 37.25) (layer F.CrtYd) (width 0.12))
    (fp_circle (center -41.25 -41.25) (end -37.25 -41.25) (layer F.CrtYd) (width 0.12))
    (fp_line (start -46 46) (end -46 -46) (layer F.Fab) (width 0.12))
    (fp_line (start 46 46) (end -46 46) (layer F.Fab) (width 0.12))
    (fp_line (start 46 -46) (end 46 46) (layer F.Fab) (width 0.12))
    (fp_line (start -46 -46) (end 46 -46) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 41.25 -41.25 270) (size 8 8) (drill 4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 41.25 41.25 180) (size 8 8) (drill 4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -41.25 41.25 90) (size 8 8) (drill 4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -41.25 -41.25) (size 8 8) (drill 4) (layers *.Cu *.Mask))
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F4E6)
    (at 255 106)
    (path /5CDA7F18)
    (fp_text reference R62 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(R61-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F4CF)
    (at 238 106)
    (path /5CDA796A)
    (fp_text reference R61 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(R61-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F4B8)
    (at 255 115)
    (path /5CDA7BB2)
    (fp_text reference R60 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(R59-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F4A1)
    (at 238 115)
    (path /5CDA70BD)
    (fp_text reference R59 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 50 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(R59-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F48A)
    (at 264 41.604721)
    (path /5CDB5737)
    (fp_text reference R58 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(R57-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F473)
    (at 247 41.604721)
    (path /5CDB5731)
    (fp_text reference R57 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(R57-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(R56-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F45C)
    (at 230 41.604721)
    (path /5CDB572B)
    (fp_text reference R56 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(R56-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F445)
    (at 264 50.784442)
    (path /5CDB5723)
    (fp_text reference R55 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(R54-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F42E)
    (at 247 50.784442)
    (path /5CDB571D)
    (fp_text reference R54 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(R54-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(R53-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F417)
    (at 230 50.784442)
    (path /5CDB5717)
    (fp_text reference R53 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(R53-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F400)
    (at 264 59.964163)
    (path /5CDAE460)
    (fp_text reference R52 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(R51-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F3E9)
    (at 247 59.964163)
    (path /5CDAE45A)
    (fp_text reference R51 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(R51-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(R50-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CDA07B6)
    (at 230 59.964163)
    (path /5CDAE454)
    (fp_text reference R50 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(R50-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F3BB)
    (at 264 69.143884)
    (path /5CDAE44C)
    (fp_text reference R49 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(R48-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F3A4)
    (at 247 69.143884)
    (path /5CDAE446)
    (fp_text reference R48 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(R48-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(R47-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F38D)
    (at 230 69.143884)
    (path /5CDAE440)
    (fp_text reference R47 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(R47-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F376)
    (at 264 78.323605)
    (path /5CDAA569)
    (fp_text reference R46 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(R45-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F35F)
    (at 247 78.323605)
    (path /5CDAA563)
    (fp_text reference R45 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(R45-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(R44-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F348)
    (at 230 78.323605)
    (path /5CDAA55D)
    (fp_text reference R44 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(R44-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F331)
    (at 264 87.503326)
    (path /5CDA8BA6)
    (fp_text reference R43 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(R42-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD9F31A)
    (at 247 87.503326)
    (path /5CDA8A1F)
    (fp_text reference R42 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(R42-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(R41-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CDA0F18)
    (at 230 87.503326)
    (path /5CDA811D)
    (fp_text reference R41 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(R41-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD9EEDC)
    (at 267 110)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CDC1336)
    (fp_text reference J6 (at 0.5 3.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD9EED0)
    (at 226 110)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CDC0510)
    (fp_text reference J5 (at 0.5 3.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD9EEC4)
    (at 285 63)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CDC1A5E)
    (fp_text reference J4 (at 0.5 3.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD9EEB8)
    (at 218 65)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CDC144C)
    (fp_text reference J3 (at 0.5 3.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A1FC)
    (at 117 132.222216)
    (path /5CD0E3BD)
    (fp_text reference R40 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(R39-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD052F5)
    (at 100 132.222216)
    (path /5CD06A9D)
    (fp_text reference R39 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(R39-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A23E)
    (at 117 123.042489)
    (path /5CD0E3B7)
    (fp_text reference R38 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(R37-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD052C7)
    (at 100 123.042489)
    (path /5CD06A97)
    (fp_text reference R37 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(R37-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A280)
    (at 117 113.862768)
    (path /5CD0E3B1)
    (fp_text reference R36 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(R35-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05299)
    (at 100 113.862768)
    (path /5CD06A91)
    (fp_text reference R35 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(R35-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A2C2)
    (at 117 104.683047)
    (path /5CD0E3AB)
    (fp_text reference R34 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(R33-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0526B)
    (at 100 104.683047)
    (path /5CD06A8B)
    (fp_text reference R33 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(R33-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A304)
    (at 117 95.503326)
    (path /5CD0E375)
    (fp_text reference R32 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(R31-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0523D)
    (at 100 95.503326)
    (path /5CD02DF3)
    (fp_text reference R31 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(R31-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A346)
    (at 117 86.323605)
    (path /5CD0E36F)
    (fp_text reference R30 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(R29-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0520F)
    (at 100 86.323605)
    (path /5CD02DED)
    (fp_text reference R29 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(R29-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A388)
    (at 117 77.143884)
    (path /5CD0E369)
    (fp_text reference R28 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R27-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD051E1)
    (at 100 77.143884)
    (path /5CD02DE7)
    (fp_text reference R27 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R27-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A40C)
    (at 117 67.964163)
    (path /5CD0E363)
    (fp_text reference R26 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(R25-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD051B3)
    (at 100 67.964163)
    (path /5CD02DE1)
    (fp_text reference R25 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(R25-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A44E)
    (at 117 58.784442)
    (path /5CD0E35D)
    (fp_text reference R24 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05185)
    (at 100 58.784442)
    (path /5CD00D29)
    (fp_text reference R23 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(R23-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A3CA)
    (at 117 49.604721)
    (path /5CD0E357)
    (fp_text reference R22 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05157)
    (at 100 49.604721)
    (path /5CD00D23)
    (fp_text reference R21 (at -0.1 0.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(R21-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05140)
    (at 54 113.862768 180)
    (path /5CD0E351)
    (fp_text reference R20 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05129)
    (at 71 113.862768 180)
    (path /5CCFEE45)
    (fp_text reference R19 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R19-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05112)
    (at 54 123.042489 180)
    (path /5CD0E34B)
    (fp_text reference R18 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD050FB)
    (at 71 123.042489 180)
    (path /5CCFE912)
    (fp_text reference R17 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R17-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD050E4)
    (at 54 132.222216 180)
    (path /5CD0E3A5)
    (fp_text reference R16 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD050CD)
    (at 71 132.222216 180)
    (path /5CD0583D)
    (fp_text reference R15 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R15-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD050B6)
    (at 54 104.683047 180)
    (path /5CD0E39F)
    (fp_text reference R14 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0509F)
    (at 71 104.683047 180)
    (path /5CD05837)
    (fp_text reference R13 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(R13-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05088)
    (at 54 95.503326 180)
    (path /5CD0E399)
    (fp_text reference R12 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05071)
    (at 71 95.503326 180)
    (path /5CD05831)
    (fp_text reference R11 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(R11-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0505A)
    (at 54 86.323605 180)
    (path /5CD0E393)
    (fp_text reference R10 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05043)
    (at 71 86.323605 180)
    (path /5CD0582B)
    (fp_text reference R9 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(R10-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0502C)
    (at 54 77.143884 180)
    (path /5CD0E38D)
    (fp_text reference R8 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD05015)
    (at 71 77.143884 180)
    (path /5CD05825)
    (fp_text reference R7 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(R7-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD04FFE)
    (at 54 67.964163 180)
    (path /5CD0E387)
    (fp_text reference R6 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD04FE7)
    (at 71 67.964163 180)
    (path /5CD0581F)
    (fp_text reference R5 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD07DF7)
    (at 54 58.784442 180)
    (path /5CD0E381)
    (fp_text reference R4 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A52F)
    (at 71 58.784442 180)
    (path /5CD05819)
    (fp_text reference R3 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(R3-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD04FA2)
    (at 54 49.604721 180)
    (path /5CD0E37B)
    (fp_text reference R2 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module custom_footprint:LTO100 (layer F.Cu) (tedit 5CD9592E) (tstamp 5CD0A4A7)
    (at 71 49.604721 180)
    (path /5CD05813)
    (fp_text reference R1 (at -0.1 0.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20 (at -0.26 -1.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.88 2.54) (end -7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end -7.88 2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start 7.88 2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (fp_line (start -7.88 -2.54) (end 7.88 -2.54) (layer F.CrtYd) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 4 5) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-2_Vertical.step
      (offset (xyz -5.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CD06633)
    (at 36 140)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CD06616)
    (at 186 140)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CD065F9)
    (at 186 40)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5CD065C7)
    (at 36 40)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD04F74)
    (at 62 140 270)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CD6A227)
    (fp_text reference J2 (at 0.5 3.2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 270) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TestPoint:TestPoint_Loop_D3.80mm_Drill2.5mm (layer F.Cu) (tedit 5A0F774F) (tstamp 5CD0B5D4)
    (at 62 40 270)
    (descr "wire loop as test point, loop diameter 3.8mm, hole diameter 2.5mm")
    (tags "test point wire loop bead")
    (path /5CD692B4)
    (fp_text reference J1 (at 0.5 3.2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x01_Female (at 0 -2.8 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.5 3.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.3 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -0.3) (end -1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start 1.9 0.3) (end 1.9 -0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 0.3) (end 1.9 0.3) (layer F.Fab) (width 0.12))
    (fp_line (start -1.9 -0.3) (end -1.9 0.3) (layer F.Fab) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 270) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D3.80mm_Drill2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 31 35) (end 191 35) (layer Edge.Cuts) (width 0.05) (tstamp 5CD05760))
  (gr_line (start 31 145) (end 31 35) (layer Edge.Cuts) (width 0.05) (tstamp 5CD07D9D))
  (gr_line (start 191 145) (end 31 145) (layer Edge.Cuts) (width 0.05) (tstamp 5CDA449B))
  (gr_line (start 191 35) (end 191 145) (layer Edge.Cuts) (width 0.05))

  (segment (start 76.08 47.359998) (end 76.08 49.604721) (width 5) (layer B.Cu) (net 1))
  (segment (start 81.439998 42) (end 76.08 47.359998) (width 5) (layer B.Cu) (net 1))
  (segment (start 90 42) (end 81.439998 42) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 49.604721) (end 94.92 46.92) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 46.92) (end 90 42) (width 5) (layer B.Cu) (net 1))
  (segment (start 79.439998 40) (end 81.439998 42) (width 5) (layer B.Cu) (net 1))
  (segment (start 73.975279 40) (end 72 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 42.104721) (end 73.975279 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 49.604721) (end 76.08 42.104721) (width 5) (layer B.Cu) (net 1))
  (segment (start 62 40) (end 72 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 72 40) (end 79.439998 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 64.828427 40) (end 62 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 92.815279 40) (end 64.828427 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 42.104721) (end 92.815279 40) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 49.604721) (end 94.92 42.104721) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 49.604721) (end 94.92 58.784442) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 49.604721) (end 76.08 58.784442) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 58.784442) (end 76.08 67.964163) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 67.964163) (end 76.08 77.143884) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 77.143884) (end 76.08 86.323605) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 86.323605) (end 76.08 95.503326) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 95.503326) (end 76.08 104.683047) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 104.683047) (end 76.08 113.862768) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 113.862768) (end 76.08 123.042489) (width 5) (layer B.Cu) (net 1))
  (segment (start 76.08 123.042489) (end 76.08 132.222216) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 58.784442) (end 94.92 67.964163) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 67.964163) (end 94.92 77.143884) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 77.143884) (end 94.92 86.323605) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 86.323605) (end 94.92 95.503326) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 95.503326) (end 94.92 104.683047) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 104.683047) (end 94.92 113.862768) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 113.862768) (end 94.92 123.042489) (width 5) (layer B.Cu) (net 1))
  (segment (start 94.92 123.042489) (end 94.92 132.222216) (width 5) (layer B.Cu) (net 1))
  (segment (start 48.92 49.604721) (end 48.92 58.784442) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 58.784442) (end 48.92 67.964163) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 67.964163) (end 48.92 77.143884) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 77.143884) (end 48.92 86.323605) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 86.323605) (end 49.323605 86.323605) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 86.323605) (end 48.92 95.503326) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 95.503326) (end 48.92 104.683047) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 104.683047) (end 48.92 113.862768) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 113.862768) (end 48.92 123.042489) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 123.042489) (end 48.92 132.222216) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 49.604721) (end 122.08 58.784442) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 58.784442) (end 122.08 67.964163) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 67.964163) (end 122.08 77.143884) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 77.143884) (end 122.08 86.323605) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 86.323605) (end 122.08 95.503326) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 95.503326) (end 122.08 104.683047) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 104.683047) (end 122.08 113.862768) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 113.862768) (end 122.08 123.042489) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 123.042489) (end 122.08 132.222216) (width 5) (layer B.Cu) (net 2))
  (segment (start 64.828427 140) (end 62 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 115.455938 140) (end 64.828427 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 133.375938) (end 115.455938 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 122.08 132.222216) (end 122.08 133.375938) (width 5) (layer B.Cu) (net 2))
  (segment (start 59.171573 140) (end 62 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 49.197784 140) (end 59.171573 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 139.722216) (end 49.197784 140) (width 5) (layer B.Cu) (net 2))
  (segment (start 48.92 132.222216) (end 48.92 139.722216) (width 5) (layer B.Cu) (net 2))
  (segment (start 65.92 49.604721) (end 59.08 49.604721) (width 5) (layer B.Cu) (net 3))
  (segment (start 59.08 77.143884) (end 65.92 77.143884) (width 5) (layer B.Cu) (net 6))
  (segment (start 59.08 86.323605) (end 65.92 86.323605) (width 5) (layer B.Cu) (net 7))
  (segment (start 59.08 95.503326) (end 65.92 95.503326) (width 5) (layer B.Cu) (net 8))
  (segment (start 65.92 104.683047) (end 59.08 104.683047) (width 5) (layer B.Cu) (net 9))
  (segment (start 59.08 132.222216) (end 65.92 132.222216) (width 5) (layer B.Cu) (net 10))
  (segment (start 59.08 123.042489) (end 65.92 123.042489) (width 5) (layer B.Cu) (net 11))
  (segment (start 59.08 113.862768) (end 65.92 113.862768) (width 5) (layer B.Cu) (net 12))
  (segment (start 111.92 49.604721) (end 105.08 49.604721) (width 5) (layer B.Cu) (net 13))
  (segment (start 105.08 58.784442) (end 111.92 58.784442) (width 5) (layer B.Cu) (net 14))
  (segment (start 111.92 67.964163) (end 105.08 67.964163) (width 5) (layer B.Cu) (net 15))
  (segment (start 105.08 77.143884) (end 111.92 77.143884) (width 5) (layer B.Cu) (net 16))
  (segment (start 111.92 86.323605) (end 105.08 86.323605) (width 5) (layer B.Cu) (net 17))
  (segment (start 105.08 95.503326) (end 111.92 95.503326) (width 5) (layer B.Cu) (net 18))
  (segment (start 111.92 104.683047) (end 105.08 104.683047) (width 5) (layer B.Cu) (net 19))
  (segment (start 105.08 113.862768) (end 111.92 113.862768) (width 5) (layer B.Cu) (net 20))
  (segment (start 111.92 123.042489) (end 105.08 123.042489) (width 5) (layer B.Cu) (net 21))
  (segment (start 105.08 132.222216) (end 111.92 132.222216) (width 5) (layer B.Cu) (net 22))

)
