(module ALFG2PF241 (layer F.Cu) (tedit 5CBD9299)
  (descr "Panasonic Relay SPST, http://www.farnell.com/datasheets/2244182.pdf")
  (tags "Panasonic Relay SPST")
  (fp_text reference REF** (at 12.1 -11.5 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ALFG2PF241 (at 12.1 3.9 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.1402 -13.97) (end -4.1402 1.9558) (layer F.Fab) (width 0.1))
  (fp_line (start -4.1402 1.9558) (end 26.162 1.9558) (layer F.Fab) (width 0.1))
  (fp_line (start 26.162 1.9304) (end 26.162 -13.97) (layer F.Fab) (width 0.1))
  (fp_line (start 9.96 -0.91) (end 9.56 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.36 -1.61) (end 9.16 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.16 -1.61) (end 9.16 -0.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.16 -0.91) (end 10.36 -0.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.36 -0.91) (end 10.36 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 26.05 -13.85) (end -4.05 -13.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.05 -13.85) (end -4.05 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.05 1.85) (end 26.05 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 26.05 1.85) (end 26.05 -13.85) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 12 -3.75 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.05 -13.85) (end 26.05 -13.85) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.05 -13.85) (end 26.05 1.85) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.05 1.85) (end -4.05 1.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.05 1.85) (end -4.05 -13.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.1402 -13.97) (end 26.1366 -13.97) (layer F.Fab) (width 0.12))
  (pad 1 thru_hole rect (at 0 0 90) (size 2.9 2.9) (drill 1.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 22 0 90) (size 2.9 2.9) (drill 1.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 24.8 -12 90) (size 3.3 3.3) (drill 2) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at -2.8 -12 90) (size 3.3 3.3) (drill 2) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/3d-models/ALFG2PF241.wrl
    (offset (xyz -4 -2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
