(module ALFG2PF241 (layer F.Cu) (tedit 5CE275E3)
  (descr "Panasonic Relay SPST, http://www.farnell.com/datasheets/2244182.pdf")
  (tags "Panasonic Relay SPST")
  (fp_text reference REF** (at 11.6 3.6 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ALFG2PF241 (at 12.1 3.9 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.1402 -13.97) (end -4.1402 1.9558) (layer F.Fab) (width 0.1))
  (fp_line (start -4.1402 1.9558) (end 26.162 1.9558) (layer F.Fab) (width 0.1))
  (fp_line (start 26.162 1.9304) (end 26.162 -13.97) (layer F.Fab) (width 0.1))
  (fp_line (start 26.05 -13.85) (end -4.05 -13.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.05 -13.85) (end -4.05 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.05 1.85) (end 26.05 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 26.05 1.85) (end 26.05 -13.85) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 12 -3.75 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.05 -13.85) (end 26.05 -13.85) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.05 -13.85) (end 26.05 1.85) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.05 1.85) (end -4.05 1.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.05 1.85) (end -4.05 -13.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.1402 -13.97) (end 26.1366 -13.97) (layer F.Fab) (width 0.12))
  (fp_circle (center 22 0) (end 30.5 0) (layer Eco1.User) (width 0.12))
  (fp_circle (center 0 0) (end 8.5 0) (layer Eco1.User) (width 0.12))
  (fp_line (start 3.5 0) (end 9.1 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.9 -11.5) (end 18.2 -11.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 -11.5) (end 12.9 -11.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -12) (end 11 -11) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -10) (end 11 -9) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -8) (end 11 -7) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -6) (end 11 -5) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -2) (end 11 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 9 -11.5) (end 12.9 -12.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 -11.5) (end 21.3 -11.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 0) (end 18.5 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.7 -11.5) (end 9 -11.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 0.7) (end 12.9 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 0.7) (end 9.1 0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.9 -0.7) (end 12.9 0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 -0.7) (end 12.9 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.1 0.7) (end 9.1 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -4) (end 11 -3) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole circle (at 0 0 90) (size 5 5) (drill oval 1 2.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 22 0 90) (size 4.5 4.5) (drill oval 1 2.2) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 24.8 -12 90) (size 5 5) (drill oval 2.2 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -2.8 -12 90) (size 5 5) (drill oval 2.2 1.5) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/3d-models/ALFG2PF241.wrl
    (offset (xyz -4 -2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
