(module rg400_solder_braid (layer F.Cu) (tedit 5CDA8850)
  (fp_text reference REF** (at 1.25 -2.75) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value rg400_solder_braid (at 1.5 3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 0 0 180) (size 4 4) (drill 1.8) (layers *.Cu *.Mask))
)
