(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "SSI2164-multiunit" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "VCA" (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "quad vca" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Quad VCA" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSI2164-multiunit_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "Iout" (effects (font (size 0.5 0.5))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "Iin" (effects (font (size 0.5 0.5))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 6.35 270) (length 3.8)
        (name "Vc" (effects (font (size 0.5 0.5))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSI2164-multiunit_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "Iout" (effects (font (size 0.5 0.5))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "Iin" (effects (font (size 0.5 0.5))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 6.35 270) (length 3.8)
        (name "Vc" (effects (font (size 0.5 0.5))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSI2164-multiunit_3_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "Iout" (effects (font (size 0.5 0.5))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "Iin" (effects (font (size 0.5 0.5))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 6.35 270) (length 3.8)
        (name "Vc" (effects (font (size 0.5 0.5))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSI2164-multiunit_4_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "Iout" (effects (font (size 0.5 0.5))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "Iin" (effects (font (size 0.5 0.5))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 6.35 270) (length 3.8)
        (name "Vc" (effects (font (size 0.5 0.5))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSI2164-multiunit_5_1"
      (rectangle (start -2.54 5.08) (end 2.54 -5.08)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (pin power_in line (at -3.81 3.81 0) (length 1.27)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 0 0) (length 1.27)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 -3.81 0) (length 1.27)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
